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Figure C -7 Typical Popout Spall Repair Detsil
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Figure C 8. Full Depth Rigid Pavement Siab Repair Detsl - Plan
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Figure C-9. Full Depth Rigid Pavement Slab Repir Detai - Section
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Figare € -2. Corner Break Repair Detail - Scction
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Figure C-3. Corner Break Repair Saw Cut Detil - Plan




